### void aufnehmen ()

Durch diese Methode wird das Aufnehmen einer Transporteinheit eingeleitet. Dazu wird für den Baustein das Ereignis ETaaufnehmen eingeplant. Hierin wird der Zustand des Bausteins auf AUFNEHMEN gesetzt, die Transporteinheit aufgenommen und in Abhängigkeit von der Aufnahmezeit das Ereignis ETeaufnehmen eingeplant.

See Also Bausteinanweisungen void arbeiten (SimTime arbZeit) void abgeben (unsigned vorgNr) void schlafen (SimTime zeit) void warten () void syncBst (unsigned bstNr) void aktivieren (unsigned bstNr, SimTime delta) void bestelleArtikel (unsigned artNr, unsigned bstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg void bestelleArbeitsplan (unsigned arbNr, unsigned bstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg) void storniereArtikel (unsigned artNr, unsigned bstNr, unsigned istVorg) void storniereArbeitsplan (unsigned arbNr, unsigned bstNr, unsigned istVorg) void zuweisenArtikel (unsigned artNr, unsigned vonBstNr, unsigned nachBstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg) void zuweisenArbeitsplan (unsigned arbNr, unsigned vonBstNr, unsigned nachBstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg)