### void aktivieren (unsigned bstNr, SimTime delta)

Für den zu aktivierenden Baustein der Nummer bstNr wird das Ereignis ETaktivieren nach der relativen Modellzeit delta [in SimTime-Format] eingeplant.

Der Übergabeparameter delta ist hierbei optional, wird er nicht definiert, wird das Ereignis sofort eingeplant.

See Also Bausteinanweisungen void aufnehmen () void arbeiten (SimTime arbZeit) void abgeben (unsigned vorgNr) void schlafen (SimTime zeit) void warten () void syncBst (unsigned bstNr) void bestelleArtikel (unsigned artNr, unsigned bstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg void bestelleArbeitsplan (unsigned arbNr, unsigned bstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg) void storniereArtikel (unsigned artNr, unsigned bstNr, unsigned istVorg) void storniereArbeitsplan (unsigned arbNr, unsigned bstNr, unsigned istVorg) void zuweisenArtikel (unsigned artNr, unsigned vonBstNr, unsigned nachBstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg) void zuweisenArbeitsplan (unsigned arbNr, unsigned vonBstNr, unsigned nachBstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg)