### void abgeben (unsigned vorgNr)

Durch diese Methode wird das Abgeben einer Transporteinheit vom aktuellen Baustein nachgebildet. Hierbei wird für den Baustein das Ereignis ETaabgeben eingeplant, der Zustand des Bausteins auf ABGEBEN gesetzt und abhängig von der Aufnahmezeit des entsprechenden Bausteins der Vorgangsnummer vorgNr das Ereignis ETeabgeben eingeplant.

Der Übergabeparameter ist optional, wird er nicht definiert, wird die Transporteinheit an den Baustein des nachfolgenden Vorgangs gemäß Arbeitsplan abgegeben.

See Also Bausteinanweisungen void aufnehmen () void arbeiten (SimTime arbZeit) void schlafen (SimTime zeit) void warten () void syncBst (unsigned bstNr) void aktivieren (unsigned bstNr, SimTime delta) void bestelleArtikel (unsigned artNr, unsigned bstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg void bestelleArbeitsplan (unsigned arbNr, unsigned bstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg) void storniereArtikel (unsigned artNr, unsigned bstNr, unsigned istVorg) void storniereArbeitsplan (unsigned arbNr, unsigned bstNr, unsigned istVorg) void zuweisenArtikel (unsigned artNr, unsigned vonBstNr, unsigned nachBstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg) void zuweisenArbeitsplan (unsigned arbNr, unsigned vonBstNr, unsigned nachBstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg)