### void arbeiten (SimTime arbZeit)

Diese Methode bildet das Bearbeiten einer Transporteinheit auf dem aktuellen Baustein nach. Dazu wird für den Baustein das Ereignis ETaarbeiten eingeplant. Hierin wird der Zustand des Bausteins auf ARBEITEN gesetzt und abhängig der Bearbeitungszeit arbZeit [in SimTime-Format] das Ereignis ETearbeiten eingeplant.

Der Übergabeparameter ist optional, wird er nicht definiert, entspricht die Bearbeitungszeit dem Wert aus dem Arbeitsplan.

See Also Bausteinanweisungen void aufnehmen () void abgeben (unsigned vorgNr) void schlafen (SimTime zeit) void warten () void syncBst (unsigned bstNr) void aktivieren (unsigned bstNr, SimTime delta) void bestelleArtikel (unsigned artNr, unsigned bstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg void bestelleArbeitsplan (unsigned arbNr, unsigned bstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg) void storniereArtikel (unsigned artNr, unsigned bstNr, unsigned istVorg) void storniereArbeitsplan (unsigned arbNr, unsigned bstNr, unsigned istVorg) void zuweisenArtikel (unsigned artNr, unsigned vonBstNr, unsigned nachBstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg) void zuweisenArbeitsplan (unsigned arbNr, unsigned vonBstNr, unsigned nachBstNr, unsigned wieoft, unsigned istVorg, unsigned sollVorg)